For full installation with a new system copy the PDF files (manuals to your desktop)  and then double click on the   INSTALLER_HT batch file then follow the prompts. Vertek also recommends copying the two Driver folders to the desktop in case of any issues with finding the ports with different data units
The FULL installation automatically loads the CDM drivers which are used with our current version of the HT-0590

For manual installation 
Run Coneplot and Cleanup installers first
Then run CPTSND installer  (DIGITAL CONE is recommended instead of CPTSND on XP computers or WIN 7 with limited ram)

Coneplot 3.0.9 is the newest version which is different from previous dated versions in look and has many enhanced features. You may wish to install this version alongside the older version to
allow time to become aclimated to the new features. If not you may install 2.7.6 only.

CPTSND 2.7.6 is a full version of our acquisition software and requires Win 7 or 10 with dot net loaded.  If you have an older computer or XP we recommend loading only the DIGITAL CONE installer as this version is set up to work with less modern computers

Some older systems may require the older Quatech drivers.Before plugging in the usb cable, make sure that the Quatech drivers folder is accessible to 
Windows.Then plug in the usb cable and give the system time to configure the drivers. If the ports do not configure correctly, go to Windows Device Manager and use the update drivers function for the port devices,
They will have Yellow exclamation points.


